So here in this document I will describe what had been implemented regarding the IoT system which basically:

* Reads a measurement from a Source (PLC/PH sensor/fake data)
* Associates the TimeStamp to it (up to miliseconds)
* Plots a window of the last X samples.
* There are buttons to stop/start the reading and send it to the cloud !
* The DDBB has some structure to alloca