

Cleaning Report IoTubes

This document contains the automatically generated report regarding the cleaning of the piping system **Piping\_C7** carried out by the cleaning machine **ID12342** the day **May 24, 2018** according to the FDA standard procedure **FDA53531984EX.** The process was carried out by: Carsten and Ole P. Ness.

# Cleaning Requirements

The requirements for the FDA cleaning procedure FDA53531984EX are exposed in the following table:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Units | Desired value | Warning Range | Error Range |
| Time | minutes | 150 | 10 | 30 |
| PH | pH | 5.3 | 2.5 | 3.2 |

# Cleaning Report

## PH report

The next Figure shows the levels of PH during the cleaning procedure.

